- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:buspower

# IO Bus Power

The IO Bus can be put to sleep allowing for power savings in low data applications.

Reset IO bus power if module lost | If enabled the RIO will reset the IO bus automatically if a module is removed.
Enable IO Bus Sleep | If this feature is enabled the RIO will turn the power to the IO bus off. If disabled the IO bus will remain powered. Power will also be maintained to the bus if there is an active GUI connection to the RIO.
Warmup Time | This is the time allotted for the modules on the IO bus to reestablish with the RIO. Allowing the RIO to acquire current values for the IO.
On Time | This is the time (after the warmup time) the RIO will maintain power to the bus after receiving a wakeup event.
Off Time | This is the time the RIO will remove power from the bus if operating in an timed interval mode. If this is set to 0 the IO bus can still be woken up by data or modbus.
Wake On Data | If there is any traffic on the selected port it will trigger a wakeup event.
Wake On Modbus | If there is a valid modbus request for the RIO's address (defined in Modbus RTU) on the selected port it will trigger a wakeup event.

rio900ns/buspower.txt · Last modified: 2022/07/08 08:41 by

### Page Tools

- Edit draft
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top