- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:comm

# Communication

## Data Communications

- Data Rate: 1200 - 115,200 Baud
- Data Interface:
  - 1 RS232 (DB9 Female)
  - 1 RS232/RS485 (2, 4 Pin Terminals)
  - 5-Pin Bus Connector for I/O Modules

## Radio Communications

- RF Band:
  - 902-928 MHz License Free
  - Spread Spectrum (North America)
  - 915-928 MHz (International version)
- RF Data Rate: 9.6 or 115.2 Kbps
- Range: (LOS) >20 miles
- Transmit Power: 100 mW - 1 Watt / 20 – 30dBm
- Receive Sensitivity:
  - -106 dBm (@LOW)
  - -103 dBm (@HIGH)
- Antenna Connector: MCX

rio900ns/comm.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top