- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:onboard

# Digital I/O

Set parameters that are used by the Device > Digital I/O function.

These are also used when the device is reset to initialize the digital outputs. If the mode is 'on/off' then on reset the digital output is set to the last values entered using Device > Digital I/O. If the mode is 'pulse' then on reset the digital output is set to the value of 'base'.

Mode | Select on/off or pulse mode.
Base | Value of signal when not being pulsed. Pulsed value is the complement of this.
Duration | Pulse duration in seconds. The digital values are set in the Internal Registers.

rio900ns/onboard.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top