- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:specs

# Specifications

## General

- Operating Temperature: -40 to +70 Deg. C
- Mounting: 30.5mm DIN rail
- Dimensions: 114.5mm (H) x 22.6mm (W) x 99mm (L)

## Electrical

- Input Voltage: +9 to 30VDC
- Max current: 4A Max (fused)
- Peak Tx Current: 86mA@24VDC / 175mA@12VDC
- Rx Current: 20mA@24VDC / 40mA@12VDC
- Isolation: >500V (RS485 bus to GND)
- Power Mode, Normal: Always On
- Relay Output: 1 Form A (SPST-NO) 75mA @ 60V Max

These ratings do not include power consumption of any attached I/O modules.

## Serial Interface

- Input/Outputs: 1 RS232 (DB9 Female), 1 RS232/isolated RS485 (terminal Blocks)
- Baud Rate: 1200-115200 Baud

## Radio

- Band: 902-928 MHz License Free
- Tx Power: 100mW - 1W, 20 – 30dBm
- Rx Sensitivity: -103 dBm (high speed) / -106 dBm (low speed)
- RF Data Rate: 110 or 250kbps
- Range (LOS): >20miles
- Antenna Connector: MCX Female

## Certification

- Regulatory: FCC, IC , ETSI
- Hazardous Location:
  - Class 1 Div II, Group C, D T3C
  - Suitable for use in: Class 1 Zone 2, IIB, T3

- FCC ID: MCQ-XBPSX
- IC ID: 1846A-XBP
- The enclosed device complies with part 15 of the FCC rules and IC ICES-003. Operation is subject to the following two conditions:
  - This device may not cause harmful interference
  - This device must accept any interference recieved including interference that may cause undesired operation.

rio900ns/specs.txt · Last modified: 2021/12/14 16:36 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top