- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:device

# Device Menu

The device menu is used to manage the attached device. The following is a description of each menu item.

## Connection Settings

Setup the parameters that will be used to connect to the device.

RIO Id | Set the id of the unit you wish to connect to. All RIOs will respond to id 0.

PC Port | Select the PC serial port that will be connected the RIO.
Detect Settings | Attempt to discover the serial parameters used by the connected device
Baud Rate | Select Baud Rate, default 9600.
Data Bits | Only 8 is supported
Parity | Select Parity to use, default N.
Stop Bits | Select number of stop bits to use, default 1.
Timeout | Set the no response timeout for the connection.
Retries | Set the number of retries to use for the connection.

IP Address | Set the IP address of the terminal server that you are using to connect to the RIO through.
Port | Set the port number of the terminal server that you are using to connect to the RIO through.
Timeout | Set the no response timeout for the connection.
Retries | Set the number of retries to use for the connection.

## Disconnect

Close the connection.

## Read Config

Read the configuration from the device.

## Write Config

Write the configuration to the device.

## Info

Read the firmware software version number, serial number and id from the device.

## Reboot

Request the device to do a reset. This is equivalent to cycling the power on the device.

rio900ns/device.txt · Last modified: 2023/08/24 14:53 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top