- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:900mbregisters

# 900MB Registers

Coils : Digital Out
Register | Description
1-8 | Outputs for the DO8 Module with the lowest address

Status : Digital In
Register | Description
1-8 | Inputs for the DI8 Module with the lowest address

Inputs : Analog In
Register | Description
1-4 | Inputs for the AI4 Module with the lowest address

Holdings : Analog
Register | Description
1-4 | Outputs for the AO4 Module with the lowest address
5-9 | Reserved
10 | Packed digital outputs
11-44 | Reserved
45 | RSSI 0-32767 → 0-5V
46 | Supply Voltage 0-32767 → 0-30V
47 | RSSI (dB)
48 | Supply Voltage (V*10)
49 | Reserved
50 | Packed digital inputs
51 | Analog Input 1 from the AI4 Module with the lowest address
52 | Analog Input 2 from the AI4 Module with the lowest address
53 | Analog Input 3 from the AI4 Module with the lowest address
54 | Analog Input 4 from the AI4 Module with the lowest address
55-62 | Reserved
63 | Counter 1-low word from the PI4 Module with the lowest address
64 | Counter 1-high word from the PI4 Module with the lowest address
65 | Counter 2-low word from the PI4 Module with the lowest address
66 | Counter 2-high word from the PI4 Module with the lowest address
67 | Counter 3-low word from the PI4 Module with the lowest address
68 | Counter 3-high word from the PI4 Module with the lowest address
69 | Counter 3-low word from the PI4 Module with the lowest address
70 | Counter 3-high word from the PI4 Module with the lowest address

rio900ns/900mbregisters.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top