- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:telemetry

# Wireless I/O Telemetry

The RIO900 is designed specially to handle situations where I/O needs to be replicated from one site to another (Figure 1). The RIO900 System can handle both point to point or point to multi-point configurations. Once a RIO900 is configured for the same RF network & I/O Telemetry Mode; Inputs from an I/O module will be mirrored at Output Module set at the same module ID (this is set by rotary switches).

Figure 1 – Point to Point I/O Telemetry

Figure 2 – Point to Multipoint I/O Telemetry

Sometimes there is a requirement not only for Point to Point to Point but also Point to Multipoint Bidirectional Telemetry. PMP I/O telemetry systems is shown below. Inputs (1) are broadcast to Outputs (1), Analog Inputs (2) are replicated as Analog Outputs (2), Digital Inputs (3) are replicated as Digital Outputs(3).

rio900ns/telemetry.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top