- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:features

# Features

- 900 MHz Unlicensed Spread Spectrum Operation (RIO900 only)
- RTU, & I/O Telemetry Operation
- RS232 and RS485 Interface
- Connect up to 8 I/O expansion modules (AI4, AO4, DI8, DO8, A8D4, COMBO-IO).
- Modbus RTU slave addressable
- End-to-End I/O telemetry using I/O expansion modules
- Fail Safe Output operation
- Link Fail Relay - can be used for alarm or shutdown

rio900ns/features.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top