- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:diagnostic

# Local Diagnostics

This displays the local diagnostic of the RIO that the GUI is connected to.

Module | This indicates the address and type of modules detected on the IO bus.
IO State | The current values of the IO.
Module Status | This is a list of current error conditions.
Telemetry Status | Indicates if telemetry is enabled or not.
Source RIO ID | The ID of the RIO that is providing the matching inputs for this module. Only applies if the local module has outputs.
Source RIO Status | Indicates the presence of an alarm condition on the associated remote RIO.
Source Module | Module type that is providing inputs to this module. Only applies if the local module has outputs.

Supply Power | Supply voltage.
Temperature | Module temperature.
Relay State | Indicates the current state of the relay.

This information will automatically update every few seconds.

rio900ns/diagnostic.txt · Last modified: 2023/08/24 16:26 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top