- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:failsafe

# Telemetry

The Telemetry section sets up the RIO for IO-IO broadcasting and fail safe applications.

Broadcast Interval | The desired interval at which the RIO will transmit the state of any inputs on the IO bus.
Force Broadcast | Send a message on the interval even if there are no modules with inputs present.
Broadcast On Change | Send a message if there is a change in the state of an input on the IO bus.
Analog Threshold | The amount of change required in an analog input to trigger a broadcast. For a 4-20mA transmitter 262 is approximately 1% of full scale. 0 to disable.
Enable IO Broadcast | Include this module when sending and receiving Telemetry messages.
Module Type | Type of output module at the indicated address. If 'DO8' or 'AO4' is selected, then a non 0 fail value can be selected.
Enable Fail safe | Enable fail safe operation for the selected module address.
Fail Value | Value to set the output to if the fail safe timeout occurs.
Timeout | The period of time without an update before the module fail safe is activated.

rio900ns/failsafe.txt · Last modified: 2022/07/18 14:34 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top