- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:registers

# Internal Registers

Coils and Status : Digitals
Register | Description
001 | Relay (0=Open, 1=Closed/Active)
002 | Low Voltage Alarm (0=Normal, 1=Alarm)
003 | Configuration Alarm (0=Normal, 1=Alarm)
004 | Telemetry Alarm (0=Normal, 1=Alarm)
005 | Failsafe Status (0=Normal, 1=Active)
006 | Com 1 Fail Status (0=Normal, 1=Alarm)
007 | Com 2 Fail Status (0=Normal, 1=Alarm)
008 | Com 3 Fail Status (0=Normal, 1=Alarm)
009 | Remote Alarm (0=Normal, 1=Alarm)
010-016 | Reserved
017-024 | Module #1 Digital Inputs
025-032 | Module #1 Digital Outputs
033-040 | Module #2 Digital Inputs
041-048 | Module #2 Digital Outputs
049-056 | Module #3 Digital Inputs
057-064 | Module #3 Digital Outputs
065-072 | Module #4 Digital Inputs
073-080 | Module #4 Digital Outputs
081-088 | Module #5 Digital Inputs
089-096 | Module #5 Digital Outputs1)
097-104 | Module #6 Digital Inputs
105-112 | Module #6 Digital Outputs
113-120 | Module #7 Digital Inputs
121-128 | Module #7 Digital Outputs
129-136 | Module #8 Digital Inputs
137-144 | Module #8 Digital Outputs
145-152 | Module #9 Digital Inputs
153-160 | Module #9 Digital Outputs
161-168 | Module #10 Digital Inputs
169-176 | Module #10 Digital Outputs
177-184 | Module #11 Digital Inputs
185-192 | Module #11 Digital Outputs
193-200 | Module #12 Digital Inputs
201-208 | Module #12 Digital Outputs
209-216 | Module #13 Digital Inputs
217-224 | Module #13 Digital Outputs
225-232 | Module #14 Digital Inputs
233-240 | Module #14 Digital Outputs
241-248 | Module #15 ESD Master Digital Inputs
249-256 | Module #15 ESD Remote Digital Outputs (249=ESD1, 250=RSD1, 251=ESD2, 252=RSD2)
257-264 | Module #16 COMBO ESD Master Digital Inputs
265-272 | Module #16 COMBO ESD Remote Digital Outputs

Holdings and Inputs: Analogs
Register | Description
001 | RIO ID
002 | Reserved
003 | Reserved
004 | Reserved
005 | Supply Voltage (V*100)
006 | Temperature (C*100)
007 | RSSI (dB)
008 | Failsafe Active2)
009-016 | Reserved
017-024 | Module #1 Analog Inputs
025-032 | Module #1 Analog Outputs
033-040 | Module #2 Analog Inputs
041-048 | Module #2 Analog Outputs
049-056 | Module #3 Analog Inputs
057-064 | Module #3 Analog Outputs
065-072 | Module #4 Analog Inputs
073-080 | Module #4 Analog Outputs
081-088 | Module #5 Analog Inputs3))
089-096 | Module #5 Analog Outputs
097-104 | Module #6 Analog Inputs
105-112 | Module #6 Analog Outputs
113-120 | Module #7 Analog Inputs
121-128 | Module #7 Analog Outputs
129-136 | Module #8 Analog Inputs
137-144 | Module #8 Analog Outputs
145-152 | Module #9 Analog Inputs
153-160 | Module #9 Analog Outputs
161-168 | Module #10 Analog Inputs
169-176 | Module #10 Analog Outputs
177-184 | Module #11 Analog Inputs
185-192 | Module #11 Analog Outputs
193-200 | Module #12 Analog Inputs
201-208 | Module #12 Analog Outputs
209-216 | Module #13 Analog Inputs
217-224 | Module #13 Analog Outputs
225-232 | Module #14 Analog Inputs
233-240 | Module #14 Analog Outputs
241-248 | Module #15 Analog Inputs
249-256 | Module #15 Analog Outputs
257-264 | Module #16 COMBO ESD Master Analog Inputs
265-272 | Module #16 COMBO ESD Remote Analog Outputs

1)
If module 5 is a PI4 module then the digital outpus are counter resets. To clear, write '0' then write PI1=89, PI2=90, PI3=91, PI4=92
2)
Bit mask of modules with active fail states. Bit 0 = Module#1, Bit 1 = Module#2
3)
If module 5 is a PI4 module then the low address is the low counter word adn the high address is the high counter word. PI1=(81,82), PI2=(83,84), PI3=(85,86), PI4=(87,88
rio900ns/registers.txt · Last modified: 2021/08/19 14:22 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top