- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:radio

# Radio

Used to set radio mode related parameters.

Site Name | Descriptor for site.
Radio Module Type | None if Radio not used, SX900 for 900 MHz
Radio Mode | Specifies the operating mode of the radio module. PEER: Standard operating mode. REPEATER: Repeater
Transmit Power | Sets the transmit power of the radio.
RF Bandwidth | Sets the over the air rate. All RIOs in the network require this parameter to be set the same.
Frequency Group | Sets the physical RF channel selection. All RIOs in the network require this parameter to be set the same.
Channel | Sets the channel number used for transmitting and receiving data between RF modules. All RIOs in the network require this parameter to be set the same.
Network ID | Network identifier. All RIOs in the network require this parameter to be set the same.
Multi Transmit Count | Sets the number of times a message will be repeated. This can improve reliability at the expense of throughput.
Network Hops | Sets the maximum number of hops a message can travel.
Enable Encryption | Enable 256bit AES Encryption on the radio module. All RIOs in the network require this parameter to be set the same.
Encryption Phrase | Set phrase used in encryption. All RIOs in the network require this parameter to be set the same.

rio900ns/radio.txt · Last modified: 2022/07/18 15:01 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top