- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:installation

# Installation

## Instructions

- Mount radio on 3.5mm DIN rail inside of an approved Type 4 enclosure.
- Attach any associated I/O Modules to DIN rail and press together to engage integrated 5 pin bus.
- Mount DIN rail end stops to prevent separation of modules.
- Wire 10-30VDC input power to RIO transceiver PWR/GND (I/O modules obtain power from bus)
- For RIO900, connect MCX antenna cable jumper to lightning arrestor and antenna cable/antenna.
- If changes in RIO configuration setting are necessary, Connect a Laptop or PC to any RIO serial port and connect to GUI software. (see software section)

rio900ns/installation.txt · Last modified: 2021/12/14 16:10 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top