- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:linkrelay

# Relay

The Relay section sets up the behavior of the relay.

Low Voltage | If the supply voltage remains below the Alarm set point for longer than the delay time the relay will open. If the supply voltage remains above the Alarm Clear set point for longer than the delay time the relay will close.
Local Configuration Error | If there is a configuration error on this unit.
Telemetry Error | If there is a configuration error between this unit and another unit.
Fail Safe Active | If the fail safe timer has expired for any attached module.
Communications Timeouts | If the unit has not received a message on the specified port within the allotted time.
Remote Alarm | If there is a known alarm that does not directly involve this unit.

rio900ns/linkrelay.txt · Last modified: 2022/07/18 15:40 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top