- skip to content

#

### User Tools

- Logged in as: ()
- Update Profile
- Admin
- Log Out

### Site Tools

- Sitemap

rio900ns:iomodules

# I/O Modules

The SCADALink I/O Modules are used to expand the I/O capabilities of the RIO by connecting to the I/O bus. Up to 10 expansion modules can be attached.

Dimensions of each module: W 0.88″ x D 3.89″ x H 4.45″

AI4 | 4 Analog Inputs (4-20mA)
AO4 | 4 Analog Outputs (4-20mA)
DI8 | 8 Digital Inputs
DO8 | 8 Digital Outputs (relays)
COMBO | 2 Digital Inputs, 2 Digital Outputs (Relays), 1 Analog Input (4-20mA), 1 Analog Output (4-20mA)
COMBO ESD MASTER (Legacy ) | Input side of COMBO ESD pair (IO same as COMBO)
COMBO ESD REMOTE (Legacy ) | Output side of COMBO ESD pair(IO same as COMBO)
ESD MASTER (Legacy ) | Input side of ESD pair. 2 Digital Inputs
ESD REMOTE (Legacy ) | Output side of ESD pair. 4 Digital Outputs (relays)

I/O Expansion Modules Bused to RIO
rio900ns/iomodules.txt · Last modified: 2023/08/24 19:27 by

### Page Tools

- Edit this page
- Backlinks
- Export to PDF
- Export Page to HTML/PDF
- Back to top